{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["size"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"size","index":0,"n_rows":24,"n_cols":40,"rows_kept":24,"cut":false,"hidden":false,"merged":[[11,12,11,17],[11,6,12,6],[2,1,2,7],[3,1,3,7],[4,1,4,7],[9,1,9,5],[9,7,9,11],[5,2,5,4],[5,8,5,9],[8,1,8,5]],"flags":["formulas_cached_only"]}
[{"$nulls":28},"AFCS80(H,V)   3/4\" Spacing 45° Curved Blade Return "]
[{"$nulls":8},"Input Data",{"$nulls":12},"Nominal Duct","Core Area","H & W",null,null," "," "]
[null,"Enter Duct Width in inches =",{"$nulls":6},18,"Inches",{"$nulls":11},"Area ( ft2 )","( ft2 )","border",null,null," Free area & Core Area Ratio",null,"Ak/Ac",1,null,null," - ",null," "]
[null,"Enter Duct Height in inches =",{"$nulls":6},18,"Inches",{"$nulls":11},2.25,2.06640625,0.75,{"$nulls":8},"\"",null,"Based on:","Titus Models 23R Return 3/4\" Spacing 45° Deflection"]
[null,"Enter Air Flow (must be greater than 0) =",{"$nulls":6},1240,"CFM",{"$nulls":22}," "]
[null,"Series =","AFCS80 H or V",{"$nulls":4},"Tag =","Room 23"]
[{"$nulls":26},"Pressure Constants",null,null,null," "]
[null,"AFCS80 H or V Return Grille",{"$nulls":25},"m","b",null," "," "]
[null,"Tag : Room 23",{"$nulls":24}," ",0,8.550295916883744]
[null,"IP Data",{"$nulls":5},"Metric Data",{"$nulls":24}," "]
[null,"Nom","Duct ","Neck","Air"," ",null,"Nom","Duct ","Neck","Air"," ",{"$nulls":19}," ","from : ","AFSC80 Sound Regression"]
[null,"Duct","Area","Vel","Flow","Ps","Nc","Duct","Area","Vel","Flow","Ps","Octave Band, dB",{"$nulls":20},"2","3","4","5","6","7","NC"]
[null,"in","ft²","FPM","CFM","\"WG",null,"mm","m²","m/s","L/s","Pa",2,3,4,5,6,7,{"$nulls":8},"Sound",{"$nulls":5},"M(An)",9.332186353829393,9.534580419240278,9.490243022534631,11.655890444991352,12.141911309535335,10.715957903684604,10.661268437525527]
[null,"18 x 18",2.25,600.0756143667297,1240,-0.16950046313895784,40.01791925772569,"457 x 457",0.20903184000000002,3.048384120982987,585.214776,-42.205615321600504,48.089766244121485,53.98414545906077,54.80071139593002,48.50136165392159,44.56070978633988,39.11460076473606,{"$nulls":10},"B","CVn","CAn",null,"M(Vn)",40.93531380103564,46.54006289701018,50.61709757475953,81.18342021365578,87.89071484724815,79.03029794718721,57.453344885408406]
[{"$nulls":26}," ",null,-122.95990624932969,57.453344885408406,10.661268437525527,null,"B",-68.57861900398431,-78.3191850234966,-88.81548535881647,-180.71702147788199,-203.4451208059607,-183.82568371377434,-122.95990624932969]
[]
[{"$nulls":27}," "]
[{"$nulls":26}," ","Band","Const","Slope 1","Slope 2"]
[{"$nulls":27},2,-68.57861900398431,40.93531380103564,9.332186353829393]
[{"$nulls":27},3,-78.3191850234966,46.54006289701018,9.534580419240278]
[{"$nulls":27},4,-88.81548535881647,50.61709757475953,9.490243022534631,{"$nulls":5}," ",null,null," "]
[{"$nulls":27},5,-180.71702147788199,81.18342021365578,11.655890444991352]
[{"$nulls":26}," ",6,-203.4451208059607,87.89071484724815,12.141911309535335]
[{"$nulls":27},7,-183.82568371377434,79.03029794718721,10.715957903684604,{"$nulls":8}," "]