{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Size"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Size","index":0,"n_rows":49,"n_cols":31,"rows_kept":49,"cut":false,"hidden":false,"merged":[[29,27,29,28],[24,27,24,28],[25,27,25,28],[26,27,26,28],[27,27,27,28],[2,1,2,7],[3,1,3,7],[4,1,4,7],[28,27,28,28],[12,10,13,10],[9,1,9,16],[11,6,11,7],[11,8,11,9],[12,11,12,16],[14,6,16,6],[35,2,37,2],[35,3,37,3],[35,4,37,4],[35,5,37,5],[35,10,37,10],[32,6,32,7],[32,8,32,9],[33,10,34,10],[35,6,37,6],[35,7,37,7],[35,8,37,8],[35,9,37,9],[30,1,30,16],[14,15,16,15],[14,16,16,16],[14,2,16,2],[14,3,16,3],[14,4,16,4],[14,5,16,5],[14,7,16,7],[14,8,16,8],[35,14,37,14],[35,15,37,15],[35,16,37,16],[33,11,33,16],[35,11,37,11],[35,12,37,12],[35,13,37,13],[5,7,5,9],[5,1,5,6],[14,13,16,13],[14,14,16,14],[14,9,16,9],[14,10,16,10],[14,11,16,11],[14,12,16,12]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":8},"Input Data",{"$nulls":11},"Nominal Duct","Core Area","H & W"]
[null,"Enter (Side A) in inches =",{"$nulls":6},12,"Inches",{"$nulls":10},"Area '( ft2 )","( ft2 )","border",null,null," - "]
[null,"Enter (Side B) in inches =",{"$nulls":6},21,"Inches",{"$nulls":10},1.75,1.75,0,null,null,"\""]
[null,"Enter Air Flow (must be greater than 0) =",{"$nulls":6},1000,"CFM",{"$nulls":10},"Area created by Side A =",null,1]
[null,"Tag = ",{"$nulls":5},"Bathroom on 4th floor",{"$nulls":17},"Throw Zones"]
[{"$nulls":26},"c(ii)","c(iii)","c(iv)"]
[{"$nulls":25},"3S  - Side A",1.8,3.58,7.01]
[null,"5SHV -  No OBD, Rectangular, 3S - Three Way Throw Pattern",{"$nulls":23},"3S  - Side B",3.29,5.27,9.04]
[null,"IP Data",{"$nulls":23},"Use 1/4 the square neck area size caused by side A for CFM calculation."]
[null,"Tag : Bathroom on 4th floor",{"$nulls":23},"Throw uses total CFM"]
[null,"Neck","Neck","Total","Total","Static","Pattern 3S Side A",null,"Pattern 3S Side B"]
[null,"Dim","Vel","Flow","Pres","Pres","flow","Throw","flow","Throw","NC","Octave Band, dB"]
[null,"in","FPM","CFM","\"WG","\"WG","CFM","ft","CFM","ft",null,2,3,4,5,6,7,{"$nulls":8},"Pressure Constants",null,null,null," "]
[null," ",571.4285714285714,1000,0.1528828600927482,0.13252562173153007,142.85714285714286,"18 - 22 - 31",428.57142857142856,"23 - 29 - 40",34.446755595206014,35.446755595206014,40.446755595206014,46.446755595206014,44.446755595206014,39.446755595206014,34.446755595206014,{"$nulls":10},"b",null," "," "]
[null,"12\" x 21\"",{"$nulls":23},"Pressure Constants",null,7.51]
[null," "]
[null,"1) Throw values are given for terminal velocities of 150, 100, and 50 fpm."]
[null,"2) Throw Values are given for Isothermal Conditions at the listed CFM per side, not total CFM."]
[null,"3) N.C. values are based on Octave Band 2 - 7 sound power levels minus a room absorption of 10dB.",{"$nulls":23},"Sound"]
[null,"4) Dash (-) in space denotes an NC or dB value of less than 10.",{"$nulls":25},"B","CVn","CAn"]
[null,"5) Data were obtained from test conducted in accordance with ANSI / ASHRAE Standard 70-1991.",{"$nulls":23},"3S",null,-133.44,60.23,7.55]
[]
[null," "]
[null," ",{"$nulls":23},"Rectangular Neck Validation:",null,"1=True, 0=False"]
[null," ",{"$nulls":23},"Height = Width?",null,0]
[null," ",{"$nulls":23},"Height or Width greater than 36",null,0]
[null," ",{"$nulls":23},"Height or Width less than 6",null,0]
[{"$nulls":25},"3\" increments?",null,0]
[null,"5SHV -  No OBD, Rectangular, 3S - Three Way Throw Pattern",{"$nulls":23},"INVALID",null,0]
[null,"Metric Data",{"$nulls":23},"SIZE"]
[null,"Tag : Bathroom on 4th floor",{"$nulls":23},"Invalid Neck Size :"]
[null,"Neck","Neck","Total","Total","Static","Pattern 3S Side A",null,"Pattern 3S Side B",{"$nulls":16},"Height can not equal Width."]
[null,"Dim","Vel","Flow","Pres","Pres","flow","Throw","flow","Throw","NC","Octave Band, dB",{"$nulls":13},"Height or Width can not be greater than 36\"."]
[null,"mm","m/s","L/s","Pa","Pa","L/s","m","L/s","m",null,2,3,4,5,6,7,{"$nulls":8},"Height or Width can not be less than 6\"."]
[null," ",2.902857142857143,471.9474,38.0678321630943,32.998879811150985,67.42105714285715,"5.5 - 6.7 - 9.5",202.26317142857144,"7.1 - 8.7 - 12.3",34.446755595206014,35.446755595206014,40.446755595206014,46.446755595206014,44.446755595206014,39.446755595206014,34.446755595206014,{"$nulls":8},"Neck must be in 3\" increments."]
[null,"305 x 533"]
[null," "]
[null,"1) Throw values are given for terminal velocities of 0.75, 0.5 and 0.25 m/s."]
[null,"2) Throw Values are given for Isothermal Conditions at the listed CFM per side, not total CFM."]
[null,"3) N.C. values are based on Octave Band 2 - 7 sound power levels minus a room absorption of 10dB."]
[null,"4) Dash (-) in space denotes an NC or dB value of less than 10."]
[null,"5) Data were obtained from test conducted in accordance with ANSI / ASHRAE Standard 70-1991."]
[]
[null," "]
[null," "]
[null," "]
[null," "]
[null," "]