{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["cfm"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"cfm","index":0,"n_rows":28,"n_cols":40,"rows_kept":28,"cut":false,"hidden":false,"merged":[[11,12,11,17],[11,6,12,6],[2,1,2,7],[3,1,3,7],[4,1,4,7],[9,1,9,5],[9,7,9,11],[5,2,5,4],[5,8,5,9],[8,1,8,5]],"flags":["formulas_cached_only"]}
[{"$nulls":28},"S480HZ or VZ Return Grille / 0 deg deflection, 3/8\" spacing"]
[{"$nulls":8},"Input Data",{"$nulls":12},"Nominal Duct","Core Area","H & W",null,null," "," "]
[null,"Enter Duct Width in inches =",{"$nulls":6},21,"Inches",{"$nulls":11},"Area ( ft2 )","( ft2 )","border",null,null," Free area & Core Area Ratio",null,"Ak/Ac",1,null,null," - ",null," "]
[null,"Enter Duct Height in inches =",{"$nulls":6},15,"Inches",{"$nulls":11},2.1875,2.00390625,0.75]
[null,"Enter Air Flow (must be greater than 0) =",{"$nulls":6},1200,"CFM",{"$nulls":22},"New Version!"]
[null,"Series =","S480 HZ or VZ",{"$nulls":4},"Tag =","R-10A"]
[{"$nulls":26},"Pressure Constants",null,null,null," ",null,"Constants from Titus 30R Catalog"]
[null,"S480 HZ or VZ Return Grille",{"$nulls":25},"m","b",null," "," "]
[null,"Tag : R-10A",{"$nulls":24},"0 deg",0,3.25,"Modified to agree with Titus"]
[null,"IP Data",{"$nulls":5},"Metric Data",{"$nulls":24}," "]
[null,"Nom","Duct ","Neck","Air"," ",null,"Nom","Duct ","Neck","Air"," ",{"$nulls":19}," ","From S480Z - Titus version sound regression.xls"]
[null,"Duct","Area","Vel","Flow","Ps","Nc","Duct","Area","Vel","Flow","Ps","Octave Band, dB",{"$nulls":20},"2","3","4","5","6","7"]
[null,"in","ft²","FPM","CFM","\"WG",null,"mm","m²","m/s","L/s","Pa",2,3,4,5,6,7,{"$nulls":8},"Sound",{"$nulls":5},"M(An)",10.20107373683118,10.201073736831187,10.201073736831223,10.20107373683145,10.201073736831662,10.210736005948204]
[null,"21 x 15",2.1875,598.8304093567251,1200,-0.050301990373036926,26.260549738351763,"533 x 381",0.2032254,3.0420584795321637,566.3368800000001,-12.525195602886194,42.45379393498773,39.30841605682255,40.04637751851813,35.577744173222506,30.799952861776205,25.751190896745314,{"$nulls":10},"B","CVn","CAn",null,"M(Vn)",44.987614680952476,37.30176468528894,36.47758021710292,54.69615336661586,74.47683562233769,78.38885999777882]
[{"$nulls":26},"0 Deg",null,-120.10858737958739,51.614937023767276,10,null,"B",-85.56995496677152,-67.36939209029781,-64.34241993509163,-119.40956656167391,-179.12432278333932,-195.04088191357454]
[]
[]
[]
[]
[]
[{"$nulls":39}," "]
[]
[{"$nulls":26}," "," "]
[{"$nulls":39}," "]
[]
[]
[]
[{"$nulls":27}," ",null,null," "]